|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CITY OF BELLE ISLE** | | | | | |
| **ITB # 21-04** | | | | | |
| **CURED IN PLACE (CIPP) FOR STORMWATER PIPE REHABILITATION** | | | | | |
| **BID FORM** | | | | | |
|  | | | | | |
| Name of Business | |  | | | |
| Contact Person | |  | | | |
| Email Address | |  | | | |
| Authorized Person Name | |  | | | |
| Signature of Authorized Person | |  | | | |
| **PROPOSED PRICING** | | | | | |
| ITEM # | DESCRIPTION | QUANTITY | UNIT | UNIT PRICE | TOTAL PRICE |
|  | **GENERAL** |  |  |  |  |
| 1 | Mobilization | 1 | LS |  |  |
| 2 | Maintenance of Traffic | 1 | LS |  |  |
|  | **Total General Bid** |  |  |  |  |
|  |  |  |  |  |  |
|  | **STORM DRAINAGE** |  |  |  |  |
| 1 | Cleaning & Video Inspection - 24” Dia. and less or equiv. | \* | LF |  |  |
| 2 | Cleaning & Video Inspection - 30” to 48” Dia. or equiv. | \* | LF |  |  |
| 3 | CIPP Liner 12” Dia. or Equiv. - 6.0 mm thickness | \* | LF |  |  |
| 4 | CIPP Liner 15” Dia. or Equiv. - 7.5 mm thickness | \* | LF |  |  |
| 5 | CIPP Liner 18” Dia. or Equiv. - 9.0 mm Thickness | \* | LF |  |  |
| 6 | CIPP Liner 24” Dia. or Equiv. - 10.5 mm Thickness | \* | LF |  |  |
| 7 | CIPP Liner 30” Dia. or Equiv. - 12.0 mm Thickness | \* | LF |  |  |
| 8 | CIPP Liner 36” Dia. Or Equiv. - 12.0 mm Thickness | \* | LF |  |  |
| 9 | CIPP Liner 42” Dia. Or Equiv. - 13.5 mm thickness | \* | LF |  |  |
| 10 | CIPP Liner 48” Dia. Or Equiv. - 15.0 mm Thickness | \* | LF |  |  |
| 11 | CIPP Liner 12” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 12 | CIPP Liner 15” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 13 | CIPP Liner 18” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 14 | CIPP Liner 24” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 15 | CIPP Liner 30” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 16 | CIPP Liner 36” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 17 | CIPP Liner 42” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 18 | CIPP Liner 48” Dia. Or Equivalent – Thickness Variance (± 1.5 mm) | \* | LF |  |  |
| 19 | Testing for Installed CIPP Liner | \* | EA |  |  |
|  | | | **Total Storm Drainage Base Bid** | |  |
|  | | |
| **TOTAL GENERAL & STORM DRAINAGE BASE BID** | | | | |  |

\* - Quantity determined on an as-needed basis.